DELTACEIR – CEIR grids by T15-T24 system

Closed “Δ” triangle shaped blade open cell ceiling system, made of aluminium, consisting of a visible substructure T15/T24 system (lay-in / lay-on) and panel elements.

The T-grid is suspended rigidly from the mounting level by means adjustable suspension hanger with 4 mm diameter. The distance between the T-profiles depends on the specified module dimension – according to the panel size length.

The edge trim is carried out by perimeter profile L, double L or C shape, 3 m long in aluminium, inner/outer same color of the panels. The height of the trim according to the panel blade height.

Pos. …..

…m² Panels – DELTACEIR – closed “Δ” triangle shaped blade ceir open cell ceiling

Type: base 4

Panel size [LxW]: …… mm (600x600 mm or 1200x600 mm)

Material thickness: ………. mm th. (0,40 mm)

Cell dimension: ………. mm (30-300 mm)

Blade height : 30 mm

Surface: ……. (plain or perforated)

Colour: ………. (white, silver, black, alu natural; others to define).

Aluminium: …….. (pre-coated, post-coated or anodised)

Unit price: ………. €/m²

Total price: ………. €

Pos. ……….

………. m² T-grid [T15/T24]

Colour: ………. (white, silver, black; other colors upon request).

Unit price: ………. €/m²

Total price: ……….

Pos. ……….

………. lm Perimeter Profile [L, double L, C]

Colour: ………. (white, silver, black; others to define)

Unit price: ………. €/lm

Total price: ……….

DELTACEIR – CEIR grids by trackless system (swing-down) type Delta system

Closed “Δ” triangle shaped blade open cell ceiling system, made of aluminium, consisting of a trackless substructure [U-shaped suspension channels] and panel elements. The system is swing-down and allows for a free-floating installation.

The U-shaped suspension channels are suspended rigidly from the mounting level by means of M6 threaded rods. The distance between the U-shaped suspension channels depends on the specified module dimension - according to the panel size length. The blades have holes for connecting the panel elements and the U-shaped suspension channels by means of springs. Each panel element is self-adjusting and can be individually hinged open.

Double cross system is possible, by means U-shaped primary and secondary suspension profiles, starting from a suspension height of 300 mm.

The edge trim (optional) is carried out by perimeter profile profile L, double L or C shape, 3 m long in aluminium, inner/outer same color of the panels. The height of the trim according to the panel blade height.

Pos. …..

…m² Panels – DELTACEIR – closed “Δ” triangle shaped blade ceir open cell ceiling

Type: base 4

Panel size [LxW]: …… mm (1200x600 mm, 600x600 mm or customized size)

Material thickness: ………. mm th. (0,40 mm)

Cell dimension: ………. mm (30-300 mm)

Blade height : 30 mm

Surface: ……. (plain or perforated)

Colour: ………. (white, silver, black, alu natural; others to define)

Aluminium: …….. (pre-coated, post-coated or anodised)

Unit price: ………. €/m²

Total price: ………. €

Pos. ……….

………. m² trackless swing-down substructure type Delta [U-shaped suspension channel]

Colour: ………. (black, others to define)

Unit price: ………. €/m²

Total price: ……….

Pos. ……….

………. lm Perimeter Profile [L, double L, C] - optional

Colour: ………. (white, silver, black; others to define)

Unit price: ………. €/lm

Total price: ……….